
|  |  |
| --- | --- |
| raspberrypilogo.jpg | Raspberry Pi |

Tutorial

Using RPi.GPIO calls on a Raspberry Pi Model 5 or Bookworm OS



Bob Rathbone Computer Consultancy

www.bobrathbone.com

Version 1.1

26th of July 2025

Contents

[Introduction 4](#_Toc192319969)

[GPIO Hardware Notes 5](#_Toc192319970)

[Conventions used in this tutorial 6](#_Toc192319971)

[Which OS works with my Raspberry Pi model 7](#_Toc192319972)

[RPi.GPIO.py 7](#_Toc192319973)

[Installation 7](#_Toc192319974)

[Installing GPIOconverter 7](#_Toc192319975)

[Installation from the ready-made package 7](#_Toc192319976)

[Uninstalling GPIOconverter package 8](#_Toc192319977)

[Installation to a local directory 8](#_Toc192319978)

[Enabling GPIO.py 8](#_Toc192319979)

[Building the GPIOconverter package 8](#_Toc192319980)

[Install the python3-lgpio package 8](#_Toc192319981)

[Downloading GPIOconverter from GitHub 9](#_Toc192319982)

[Build the GPIOconverter package 9](#_Toc192319983)

[Installing the GPIOconverter package 9](#_Toc192319984)

[Known Issues 9](#_Toc192319985)

[GPIO.setwarnings call limitations 9](#_Toc192319986)

[GPIO.cleanup does not clear used GPIOs 9](#_Toc192319987)

[Using GPIOconverter with Rotary Encoders 10](#_Toc192319988)

[Support 11](#_Toc192319989)

[Source files 11](#_Toc192319990)

[The GPIO.py shim software 11](#_Toc192319991)

[The test\_pwm.py program 11](#_Toc192319992)

[The test\_group.py program 12](#_Toc192319993)

[The .gpioconverter file 12](#_Toc192319994)

[Appendix A Licences 13](#_Toc192319995)

[Acknowledgements 13](#_Toc192319996)

[Appendix B - The RP1 general purpose I/O Chip 14](#_Toc192319997)

[Glossary 15](#_Toc192319998)

**Figures**

[Figure 1 The Raspberry Pi Model 5 RP1 I/O chip 4](#_Toc192319999)

[Figure 2 GPIO and other Headers Information 5](#_Toc192320000)

[Figure 3 The RP1 General Purpose I/O Chip 14](#_Toc192320001)

# Introduction

The Raspberry Pi Model 5 was introduced at the end of 2023. It only works with **Raspberry Pi Bookworm OS** or later.


However, the biggest impact for most developers is that the **RPi.GPIO** input/output library does not work on the **Raspberry Pi model 5** or on systems running **Bookworm**. This is because the **RPi Model** 5 now has a separate chip called **RP1** for controlling I/O including the pins on the GPIO header (**j8**). In the case of Bookworm, the authors of **RPi/GPIO** have apparently not yet updated their software (this will no doubt change in the future). This means that hundreds of thousands of programs or maybe even millions of programs need to be modified to use one of the newer libraries such as **gpiod** or **lgpio**. The **RP1** chip also controls USB ports, Gigabyte Ethernet, MIPI Camera Controllers and Low Speed Peripherals compatible with earlier versions of the Raspberry Pi.

My own product, the **Raspberry Pi Internet Radio** is also such a program and would have meant a lot of work to convert all the GPIO routines to say **GPIOD** which does run on the **RPi Model 5**. So, I decided to write a simple interface called **GPIOconverter** which converts **RPi.GPIO** calls to one of the newer **GPIO** interfaces. This is a so-called **software shim**. See the following link for more information: **https://en.wikipedia.org/wiki/Shim\_(computing)**. I eventually settled on using the excellent **python3-lgpio** library for the **GPIOconverter** software. **GPIOconverter** has been successfully tested on **LEDs, LCD's, Stepper Motors** and **Rotary encoders** (**KY-040, COM-09117** and **PEC11R** series). The architecture of the interface is shown below:

**OUTPUT: User Program --> GPIO calls --> GPIOconverter --> LGPIO**

**INPUT: LGPIO events --> GPIOconverter --> User Program even handlers**

The following illustration shows the location of the RPP1 I/O chip.



The RP1

I/O Chip

Figure The Raspberry Pi Model 5 RP1 I/O chip

See *Appendix B - The RP1 general purpose I/O Chip* on page 14 for more information.

The latest version of Bookworm is now provided with a **python3-rpi-lgpio** package as a direct drop in for **RPi.GPIO** however I still experienced problems with Rotary Encoder support so I continue to us **GPIOconverter** which can be used as an alternative to **python3-rpi-lgpio**.

# GPIO Hardware Notes




Figure 2 GPIO and other Headers Information

# Conventions used in this tutorial

Installation of the radio program requires you to enter lines at the command line prompt. This requires you to log into the Raspberry PI as user ‘**pi**’. The default password is **raspberry**.

**Note:** Don’t carry out any of the following commands just yet. They are just examples.

Raspberrypi login: **pi**

Password: **raspberry**

pi@raspberrypi:~$ Last login: Sun Apr 6 10:18:18 2014 from 192.168.2.100

pi@raspberrypi:~$

The prompt line is displayed ending with a **$** sign. The **pi@raspberrypi:~** string means user ‘pi’ on host machine called ‘raspberrypi’. The ~character means the user ‘pi’ home directory **/home/pi**. In this tutorial if you are required to do something as user **pi** then only the $ sign will be shown followed by the command as shown in the example below:

$ **pinout**

Some commands produce output which does not need to be shown. In such a case a ‘:’ is used to indicate that some output has been omitted.

**$ pinout**

Description : Raspberry Pi 5B rev 1.0

Revision : c04170

: {Output ommited}

J8:

3V3 (1) (2) 5V

GPIO2 (3) (4) 5V

GPIO3 (5) (6) GND

GPIO4 (7) (8) GPIO14

GND (9) (10) GPIO15

GPIO17 (11) (12) GPIO18

GPIO27 (13) (14) GND

GPIO22 (15) (16) GPIO23

3V3 (17) (18) GPIO24

GPIO10 (19) (20) GND

GPIO9 (21) (22) GPIO25

GPIO11 (23) (24) GPIO8

GND (25) (26) GPIO7

GPIO0 (27) (28) GPIO1

GPIO5 (29) (30) GND

GPIO6 (31) (32) GPIO12

GPIO13 (33) (34) GND

GPIO19 (35) (36) GPIO16

GPIO26 (37) (38) GPIO20

GND (39) (40) GPIO21

For further information, please refer to https://pinout.xyz/

END OF EXAMPLE COMMANDS.

# Which OS works with my Raspberry Pi model

The following article contains a table showing which model Raspberry Pi’s work with which Raspberry Pi OS: <https://en.wikipedia.org/wiki/Raspberry_Pi_OS>

# RPi.GPIO.py

The **GPIO.py code** is only for use with the **Raspberry Pi Model 5** or for earlier models such as the **Model 3B** or **4B** which are running the **Bookworm 32 or 64-bit** **OS** or later. The code is designed to intercept traditional GPIO calls and convert them to LGPIO calls. See: <https://abyz.me.uk/lg/py_lgpio.html>

|  |  |
| --- | --- |
| note_icon.png | **NOTE:** On the **15th of March 2024** the **Raspberry Pi Foundation** released a new version of the **Bookworm** Operating System Firmware which completely broke the input functionality of the GPIO header pins on the **32-Bit** version of the OS. The **64-Bit** version is still OK at the time of writing. The error manifests itself as “Error: GPIO *nn* Failed to add edge detection” where *nn* is the GPIO number of the relevant pin. However, the **GPIO.py** program now supports the **gpiochip0** circuitry embedded in the BCM processor. Once **GPIOconverter** is enable it intercepts calls to **RPi.GPIO** and converts them to **lgpio** calls. This only works on **Bookworm** or later. Earlier versions of the OS such as **Bullseye** cancontinue to use the legacy **RPi.GPIO** calls as normal. |

# Installing GPIOConverter

There are two methods of installing **GPIOconverter** software:

1. Install as a systemwide package usually in **/usr/lib/python3/dist-packages/RPi**
2. In the project directory as your **GPIO** program as a local package

**Method 2** means that only your local **RPi.GPIO** program(s) will be using **GPIOconverter**. All other system-wide GPIO programs will use the standard GPIO library in **/usr/lib/python3/dist-packages/RPi**

## Installation from the ready-made package

You can install the ready-made package from the [https://bobrathbone.com](https://bobrathbone.com/) Web site. Log into your Raspberry Pi and run the following.

sudo apt install python3-lgpio

curl -L -O https://bobrathbone.com/raspberrypi/packages/gpioconverter\_1.1\_all.deb

sudo dpkg -i gpioconverter\_1.1\_all.deb

**Note:** The **GPIOconverter** package can only be installed on **Bookworm OS** or later and isn’t required on earlier versions of the OS such as **Bullseye**.

## Uninstalling GPIOconverter package

Run the following instruction:

$ sudo dpkg -r gpioconverter

Now restore the standard **RPi.GPIO library**

$ sudo mv /usr/lib/python3/dist-packages/RPi\_standard /usr/lib/python3/dist-packages/RPi

## Installation to a local directory

It may well be that you only wish to install the package **GPIOconverter** software in a specific project directory leaving the rest of the system unaffected. If so, you do not need to create the package but only copy the main files to your project directory.

Create a sub-directory called RPi in the directory where your GPIO code is installed. For example code in directory **/usr/share/myproject**:

$ cd /usr/share/myproject

$ mkdir RPi

$ cp /home/<user>/GPIOconverter/RPi/GPIO.py /usr/share/myproject/RPi/.

Where **<user>** is your log in name (usually 'pi')

## Enabling GPIO.py

If running on a **Raspberry Pi model 5** or if running **Bookworm (32-bit)** or later. Example:

$ touch /usr/share/myproject/RPi/\_\_init\_\_.py

The above instruction will cause the code using the GPIO calls to see directory **RPi** as a package. For earlier models such as the 3B or 4 disable the package unless running on **Bookworm 32-bit OS** using the instruction below:

$ rm /usr/share/myproject/RPi/\_\_init\_\_.py

|  |  |
| --- | --- |
| note_icon.png | **NOTE:**  The first part of the above procedure is not necessary if you installed the software from the Debian package (**gpioconverter\_1.1\_all.deb**) as the installation process does this for you. |

# Building the GPIOconverter package

This is for developers only. The software is installed from the **GPIOconverter** package (gpioconverter\_1.1\_all.deb). To build it carry out the following procedure:

## Install the python3-lgpio package

The **GPIOconverter** package requires the **python3-lgpio** module. Log into the Raspberry Pi and install the **python3-lgpio** package

$ sudo apt install python3-lgpio

## Downloading GPIOconverter from GitHub

Now clone the **GPIOconverter** software to your home directory and run:

$ cd

$ git clone https://github.com/bobrathbone/GPIOconverter

## Build the GPIOconverter package

$ cd GPIOconverter

$ chmod +x build.sh

$ ./build.sh

The build script will now create the **GPIOconverter** package. Towards the end of the build you will be asked if you wish to check the package with Lintian. This is only used by developers so - Answer n

Check using Lintian y/n: n

## Installing the GPIOconverter package

At the end of the run the build script will display the instruction to install the package using **dpkg** installer as shown below:

Install the gpioconverter\_1.1\_all.deb package with the following command:

**sudo dpkg -i gpioconverter\_1.1\_all.deb**

# Known Issues

## GPIO.setwarnings call limitations

The call **GPIO.setwarnings(True|False)** is currently not implemented in a compatible manner in **lgpio**. The **lgpio** package does not have the equivalent of **GPIO.setwarnings** but has the **lgpio.exceptions** call which can be set to True or False. So, the **setwarnings** call can either be ignored or be used to enable and disable **lgpio** exceptions. Set **IGNORE\_WARNINGS** to **True** at the beginning of the **GPIO.py** program to prevent **lgpio exceptions** or control this with the **GPIO.setwarnings** call.

## GPIO.cleanup does not clear used GPIOs

The **GPIO.cleanup()** call in the standard **RPi.GPIO** package normally clears all of GPIOs used in a run.

When using **GPIOconverter** it calls the **lgpio.gpiochip\_close(chip)** routine. However, **lgpio.gpiochip\_close** does not clear the GPIOs used. To overcome this problem, you can call **GPIO.cleanup** with a list containing the used GPIOs as shown in the example below.

chan\_list = [18,16,17,4]

GPIO.cleanup(chan\_list)

Or for a single GPIO

GPIO.cleanup(16)

If you run the following this will close the I/O chip but leave the GPIOs that were used in their current state.

GPIO.cleanup()

This could be a problem if you are running say a stepper motor which might leave a winding with power on it which might lead to overheating.

## Using GPIOconverter with Rotary Encoders

There is a lot of Python software for Rotary Encoders which was originally written by Ben Buxton in 2011. You may find that the Rotary Encoder is sluggish and misses a high number of turns. In the case of the Ben Buxton code this can be corrected by changing the **HALF\_STEP** flag from **False** to **True**.

# Enable this to emit codes twice per step.

# HALF\_STEP == True: emits a code at 00 and 11

# HALF\_STEP == False: emits a code at 00 only

HALF\_STEP = True

STATE\_TAB = HALF\_TAB if HALF\_STEP else FULL\_TAB

Fortunately, the above change doesn’t seem to affect operation when running the code using the standard **RPi.GPIO** calls on say a Raspberry Pi **Model 4B**.

# Support

It is not possible to provide support for the standard **RPi.GPIO library** as literally hundreds of thousands of programs are using **RPi.GPIO** routines. The code is provided as is and without any warranties or "fit for purpose" etc. However, do contact [bob@bobrahbone.com](mailto:bob@bobrahbone.com) or raise an issue on <https://github.com/bobrathbone/GPIOconverter> for any errors or missing features found in the **GPIOconverter** software.

# Source files

As already mentioned the software is stored on **GitHub** at <https://github.com/bobrathbone/GPIOconverter>

## The GPIO.py shim software

The **GPIO.py** file uses the Python 3 LGPIO library (python3-lgpio) to handle calls to and from the RP1 i/o chip. More information on LGPIO see: <https://abyz.me.uk/lg/py_lgpio.html>

Python code examples will be found at: <https://abyz.me.uk/lg/examples.html#Python%20lgpio>

## The test\_pwm.py program

The **test\_pwm.py** program tests the **PWM** (Pulse-Width Modulation) function of **RPi.GPIO** which, which is a technique for creating variable-width pulses to encode or modulate a signal. PWM is used in many applications, including power supplies, DC-DC switching regulators, and DC motor control or in this case to brighten and dim a LED. To use it, amend the “led = 16” statement in the source code The test\_pym.py program

First edit the **test\_pwm.py** file and change the led GPIO setting to the the GPIO number you are using for the test.

# Change the following values to suit your system

Led = 16 # Led GPIO for mode BCM

Now run the program. The selected LED should brighten and dim. Press Ctrl-C to end the test.

cd /usr/share/myproject/RPi

./test\_pwm.py

**Note:** If you are only using **GPIOconverter** in a local project directory then it is necessary to first copy **test\_pwm.py** to it and run it from there as shown in the following example.

cd /usr/share/myproject

cp RPi/test\_pwm.py .

./test\_pwm.py

The above isn’t necessary if you installed the **GPIOconverter** package as previously shown.

## The test\_group.py program

The **test\_group.py** program is a simple test program used to test the **RPi.GPIO group** functions.

First edit the **test\_group.py** file and change the list of GPIOs in **chan\_list** parameter to change the GPIO list that you are using for the test.

chan\_list = [18,16,17,4] # Group GPIOs for mode BCM

chan\_list\_board = [12,36,11,7] # Group GPIOs for mode BOARD

If you are using mode **GPIO.BOARD** then also edit the **chan\_list\_board** definition. The mapping between **GPIO.BCM** and **GPIO.BOARD** will be found in the **pins** definition in **RPi.GPIO.py**

# pins is the mapping between GPIO.BOARD and GPIO.BCM. Format Pin:GPIO

pins = {

3:2, 5:3, 7:4, 8:14, 10:15, 11:17, 12:18, 13:27, 15:22, 16:23, 18:24, 19:10,

21:9, 22:25, 23:11, 24:8, 26:7, 27:0, 28:1, 29:5, 31:6, 32:12, 33:13, 35:19,

36:16, 37:26, 38:20, 40:21,

}

The program first flashes a single LED as configured by the **led** parameter and then switches alternate LEDs on and off as defined in **chan\_list** and then closes the program.

**Note:** If you are only using **GPIOconverter** in a local project directory then it is necessary to first copy **test\_group.py** to it and run it from there as shown in the following example.

cd /usr/share/myproject

cp RPi/group\_pwm.py .

./group\_pwm.py

The above isn’t necessary if you installed the **GPIOconverter** package as previously shown.

## The .gpioconverter file

In the **RPi** directory you will see a file called “**.gpioconverter”**.

$ **ls -la RPi/**

:

-rw-r--r-- 1 pi pi 0 Feb 17 13:44 .gpioconverter

:

This file is used during package installation only to check if **GPIOconverter** has been previously installed in the **/usr/lib/python3/dist-packages** directory.

If it doesn’t find this file it will know that the standard **RPi** package is still installed. It will rename the standard RPi package as **RPi-standard** and then install **GPIOconverter RPi** software in its place.

If it does find this file it will know that this is an upgrade and overwrite the contents of **/usr/lib/python3/dist-packages/RPi** with the upgrade.

# Appendix A Licences and Disclaimer

The software and documentation for this project is released under the GNU General Public Licence.

The GNU General Public License (GNU GPL or GPL) is the most widely used free software license, which guarantees end users (individuals, organizations, companies) the freedoms to use, study, share (copy), and modify the software. Software that ensures that these rights are retained is called free software. The license was originally written by Richard Stallman of the Free Software Foundation (FSF) for the GNU project.

The GPL grants the recipients of a computer program the rights of the Free Software Definition and uses *copyleft* to ensure the freedoms are preserved whenever the work is distributed, even when the work is changed or added to. The GPL is a *copyleft* license, which means that derived works can only be distributed under the same license terms. This is in distinction to permissive free software licenses, of which the BSD licenses are the standard examples. GPL was the first *copyleft* license for general use.

See <http://www.gnu.org/licenses/#GPL> for further information on the GNU General Public License.

The licences for the source and documentation for this project are:

GNU General Public License. See <http://www.gnu.org/licenses/gpl.html>

GNU AFFERO General Public License. See <http://www.gnu.org/licenses/agpl.html>

GNU Free Documentation License. See <http://www.gnu.org/licenses/fdl.html>

## Disclaimer

THIS SOFTWARE AND DOCUMENTATION IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS 'AS IS' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BELIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS, PENALTIES FOR UNAUTHORISED USE; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE OR DOCUMENTATION, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

# Acknowledgements

The people at <https://abyz.me.uk/lg/index.html>. who produced the **lgpio** package. No individuals are mentioned by name on their Web site but whoever they are, they have made an excellent product for General Purpose Input Output control on Linux Single Board Computers such as the Raspberry Pi Model 5 with extremely professional documentation. My compliments.

The GitHub member known only by the handle **fgmnts** who kindly implemented PWM support in **GPIOconverter**. See <https://github.com/fgmnts>

# Appendix B - The RP1 general purpose I/O Chip

The RP1 general purpose I/O chip is a 12×12mm, 0.65mm-pitch BGA southbridge, which provides the majority of the I/O capabilities for Raspberry Pi 5.




Figure The RP1 General Purpose I/O Chip

The RPi chip provides:

* 4-lane PCIe 2.0 endpoint
* Gigabit Ethernet MAC
* 2× USB 3 host controllers
  + Each has 1× USB 3 and 1× USB 2 port
  + More than twice the usable USB bandwidth vs. Raspberry Pi 4
* 2× SDIO ports/eMMC (not used on Raspberry Pi 5)
* 2× MIPI transceivers (4-lane, supporting DSI and CSI-2)
* Video DAC (3-channel, supporting PAL/NTSC and VGA)
  + Only one channel (composite) used on Raspberry Pi 5
* Low-speed peripherals (SPI, UART, I2C, PWM, GPIO, I2S)
* Delta-sigma PWM audio out

More information on RP1 can be found in the RP1 Peripherals document.

See <https://datasheets.raspberrypi.com/rp1/rp1-peripherals.pdf>

# Glossary

**BGA** Ball Grid Array – A popular surface mount for Integrated Circuits (ICs)

**CSI** Camera Serial Interface

**DAC** Digital to Analogue Converter (In this case for audio output cards)

**DSI**  Display Serial Interface

**GND** Ground, 0 Volts

**GPIO** General Purpose IO (On the Raspberry PI)

**I2C** Two-wire serial communication protocol

**I2S** Electrical serial bus for connecting digital audio devices

**PWM** Pulse-Width Modulation

**RP1** Input Output Controller Chip for Raspberry Pi Model 5 peripherals

**SPI** Serial Peripheral Interface – Interface us between digital components

**USB** Universal Serial Bus